<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="QFP50P1200X1200X160-64N">
</package>
<package name="QFP50P1600X1600X160-100N">
</package>
<package name="TSSOP48">
</package>
<package name="SSOP48DL">
<description>&lt;B&gt;Shrink Small Outline Package&lt;/b&gt;</description>
</package>
<package name="ESP-12-WIFI_MODULE">
</package>
</packages>
<symbols>
<symbol name="STM32F107RCT6">
<pin name="VBAT" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST"/>
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PD0_OSC_IN"/>
<pin name="PD2"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PD1_OSC_OUT"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13-TAMPER-RTC"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
</symbol>
<symbol name="STM32F107VCT6">
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA_8"/>
<pin name="PA_9"/>
<pin name="PA_10"/>
<pin name="PA_11"/>
<pin name="PA_12"/>
<pin name="PA_13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VREF-" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="OSC_IN" direction="in"/>
<pin name="NRST"/>
<pin name="NC" direction="nc"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13-TAMPER-RTC"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="STM32F745VG">
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA_8"/>
<pin name="PA_9"/>
<pin name="PA_10"/>
<pin name="PA_11"/>
<pin name="PA_12"/>
<pin name="PA_13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="OSC_IN" direction="in"/>
<pin name="NRST"/>
<pin name="VCAP2" direction="nc"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13-TAMPER-RTC"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="STM32F445XCXE">
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA_8"/>
<pin name="PA_9"/>
<pin name="PA_10"/>
<pin name="PA_11"/>
<pin name="PA_12"/>
<pin name="PA_13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11/VCAP1"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VSSA/VREF-" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="OSC_IN" direction="in"/>
<pin name="NRST"/>
<pin name="VCAP2" direction="nc"/>
<pin name="VDD_0" direction="pwr"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VSS_2" direction="pwr"/>
<pin name="VSS_3" direction="pwr"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13-TAMPER-RTC"/>
<pin name="PC14-OSC32_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="OSC_OUT" direction="out"/>
</symbol>
<symbol name="7416244">
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="3G" direction="in" function="dot"/>
<pin name="4G" direction="in" function="dot"/>
<pin name="1Y1" direction="hiz"/>
<pin name="1Y2" direction="hiz"/>
<pin name="1Y3" direction="hiz"/>
<pin name="1Y4" direction="hiz"/>
<pin name="2Y1" direction="hiz"/>
<pin name="2Y2" direction="hiz"/>
<pin name="2Y3" direction="hiz"/>
<pin name="2Y4" direction="hiz"/>
<pin name="3Y1" direction="hiz"/>
<pin name="3Y2" direction="hiz"/>
<pin name="3Y3" direction="hiz"/>
<pin name="3Y4" direction="hiz"/>
<pin name="4Y1" direction="hiz"/>
<pin name="4Y2" direction="hiz"/>
<pin name="4Y3" direction="hiz"/>
<pin name="4Y4" direction="hiz"/>
<pin name="1A1" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1A4" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="2A4" direction="in"/>
<pin name="3A1" direction="in"/>
<pin name="3A2" direction="in"/>
<pin name="3A3" direction="in"/>
<pin name="3A4" direction="in"/>
<pin name="4A1" direction="in"/>
<pin name="4A2" direction="in"/>
<pin name="4A3" direction="in"/>
<pin name="4A4" direction="in"/>
</symbol>
<symbol name="4PWR8GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="ESP-12-WIFI_MODULE">
<pin name="RST"/>
<pin name="ADC"/>
<pin name="EN"/>
<pin name="GPIO16"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="VCC"/>
<pin name="GPIO15"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="RXD0"/>
<pin name="TXD0"/>
<pin name="MOSI"/>
<pin name="CS0"/>
<pin name="MISO"/>
<pin name="GPIO9"/>
<pin name="GPIO10"/>
<pin name="SCLK"/>
<pin name="GND"/>
</symbol>
<symbol name="+5VSB">
<pin name="+5VSB" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STM32F107RCT6" prefix="U">
<description>ARM-based 32-bit MCU</description>
<gates>
<gate name="A" symbol="STM32F107RCT6"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X160-64N">
<connects>
<connect gate="A" pin="BOOT0" pad="60"/>
<connect gate="A" pin="NRST" pad="7"/>
<connect gate="A" pin="PA0-WKUP" pad="14"/>
<connect gate="A" pin="PA1" pad="15"/>
<connect gate="A" pin="PA10" pad="43"/>
<connect gate="A" pin="PA11" pad="44"/>
<connect gate="A" pin="PA12" pad="45"/>
<connect gate="A" pin="PA13" pad="46"/>
<connect gate="A" pin="PA14" pad="49"/>
<connect gate="A" pin="PA15" pad="50"/>
<connect gate="A" pin="PA2" pad="16"/>
<connect gate="A" pin="PA3" pad="17"/>
<connect gate="A" pin="PA4" pad="20"/>
<connect gate="A" pin="PA5" pad="21"/>
<connect gate="A" pin="PA6" pad="22"/>
<connect gate="A" pin="PA7" pad="23"/>
<connect gate="A" pin="PA8" pad="41"/>
<connect gate="A" pin="PA9" pad="42"/>
<connect gate="A" pin="PB0" pad="26"/>
<connect gate="A" pin="PB1" pad="27"/>
<connect gate="A" pin="PB10" pad="29"/>
<connect gate="A" pin="PB11" pad="30"/>
<connect gate="A" pin="PB12" pad="33"/>
<connect gate="A" pin="PB13" pad="34"/>
<connect gate="A" pin="PB14" pad="35"/>
<connect gate="A" pin="PB15" pad="36"/>
<connect gate="A" pin="PB2" pad="28"/>
<connect gate="A" pin="PB3" pad="55"/>
<connect gate="A" pin="PB4" pad="56"/>
<connect gate="A" pin="PB5" pad="57"/>
<connect gate="A" pin="PB6" pad="58"/>
<connect gate="A" pin="PB7" pad="59"/>
<connect gate="A" pin="PB8" pad="61"/>
<connect gate="A" pin="PB9" pad="62"/>
<connect gate="A" pin="PC0" pad="8"/>
<connect gate="A" pin="PC1" pad="9"/>
<connect gate="A" pin="PC10" pad="51"/>
<connect gate="A" pin="PC11" pad="52"/>
<connect gate="A" pin="PC12" pad="53"/>
<connect gate="A" pin="PC13-TAMPER-RTC" pad="2"/>
<connect gate="A" pin="PC14-OSC32_IN" pad="3"/>
<connect gate="A" pin="PC15-OSC32_OUT" pad="4"/>
<connect gate="A" pin="PC2" pad="10"/>
<connect gate="A" pin="PC3" pad="11"/>
<connect gate="A" pin="PC4" pad="24"/>
<connect gate="A" pin="PC5" pad="25"/>
<connect gate="A" pin="PC6" pad="37"/>
<connect gate="A" pin="PC7" pad="38"/>
<connect gate="A" pin="PC8" pad="39"/>
<connect gate="A" pin="PC9" pad="40"/>
<connect gate="A" pin="PD0_OSC_IN" pad="5"/>
<connect gate="A" pin="PD1_OSC_OUT" pad="6"/>
<connect gate="A" pin="PD2" pad="54"/>
<connect gate="A" pin="VBAT" pad="1"/>
<connect gate="A" pin="VDDA" pad="13"/>
<connect gate="A" pin="VDD_1" pad="32"/>
<connect gate="A" pin="VDD_2" pad="48"/>
<connect gate="A" pin="VDD_3" pad="64"/>
<connect gate="A" pin="VDD_4" pad="19"/>
<connect gate="A" pin="VSSA" pad="12"/>
<connect gate="A" pin="VSS_1" pad="31"/>
<connect gate="A" pin="VSS_2" pad="47"/>
<connect gate="A" pin="VSS_3" pad="63"/>
<connect gate="A" pin="VSS_4" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="STM32F107RCT6"/>
<attribute name="OC_FARNELL" value="1737139"/>
<attribute name="OC_NEWARK" value="25R9444"/>
<attribute name="PACKAGE" value="LQFP-64"/>
<attribute name="SUPPLIER" value="STMicroelectronics"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F107VCT6" prefix="U">
<description>ARM-based 32-bit MCU</description>
<gates>
<gate name="A" symbol="STM32F107VCT6"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X160-100N">
<connects>
<connect gate="A" pin="BOOT0" pad="94"/>
<connect gate="A" pin="NC" pad="73"/>
<connect gate="A" pin="NRST" pad="14"/>
<connect gate="A" pin="OSC_IN" pad="12"/>
<connect gate="A" pin="OSC_OUT" pad="13"/>
<connect gate="A" pin="PA0-WKUP" pad="23"/>
<connect gate="A" pin="PA1" pad="24"/>
<connect gate="A" pin="PA14" pad="76"/>
<connect gate="A" pin="PA15" pad="77"/>
<connect gate="A" pin="PA2" pad="25"/>
<connect gate="A" pin="PA3" pad="26"/>
<connect gate="A" pin="PA4" pad="29"/>
<connect gate="A" pin="PA5" pad="30"/>
<connect gate="A" pin="PA6" pad="31"/>
<connect gate="A" pin="PA7" pad="32"/>
<connect gate="A" pin="PA_10" pad="69"/>
<connect gate="A" pin="PA_11" pad="70"/>
<connect gate="A" pin="PA_12" pad="71"/>
<connect gate="A" pin="PA_13" pad="72"/>
<connect gate="A" pin="PA_8" pad="67"/>
<connect gate="A" pin="PA_9" pad="68"/>
<connect gate="A" pin="PB0" pad="35"/>
<connect gate="A" pin="PB1" pad="36"/>
<connect gate="A" pin="PB10" pad="47"/>
<connect gate="A" pin="PB11" pad="48"/>
<connect gate="A" pin="PB12" pad="51"/>
<connect gate="A" pin="PB13" pad="52"/>
<connect gate="A" pin="PB14" pad="53"/>
<connect gate="A" pin="PB15" pad="54"/>
<connect gate="A" pin="PB2" pad="37"/>
<connect gate="A" pin="PB3" pad="89"/>
<connect gate="A" pin="PB4" pad="90"/>
<connect gate="A" pin="PB5" pad="91"/>
<connect gate="A" pin="PB6" pad="92"/>
<connect gate="A" pin="PB7" pad="93"/>
<connect gate="A" pin="PB8" pad="95"/>
<connect gate="A" pin="PB9" pad="96"/>
<connect gate="A" pin="PC0" pad="15"/>
<connect gate="A" pin="PC1" pad="16"/>
<connect gate="A" pin="PC10" pad="78"/>
<connect gate="A" pin="PC11" pad="79"/>
<connect gate="A" pin="PC12" pad="80"/>
<connect gate="A" pin="PC13-TAMPER-RTC" pad="7"/>
<connect gate="A" pin="PC14-OSC32_IN" pad="8"/>
<connect gate="A" pin="PC15-OSC32_OUT" pad="9"/>
<connect gate="A" pin="PC2" pad="17"/>
<connect gate="A" pin="PC3" pad="18"/>
<connect gate="A" pin="PC4" pad="33"/>
<connect gate="A" pin="PC5" pad="34"/>
<connect gate="A" pin="PC6" pad="63"/>
<connect gate="A" pin="PC7" pad="64"/>
<connect gate="A" pin="PC8" pad="65"/>
<connect gate="A" pin="PC9" pad="66"/>
<connect gate="A" pin="PD0" pad="81"/>
<connect gate="A" pin="PD1" pad="82"/>
<connect gate="A" pin="PD10" pad="57"/>
<connect gate="A" pin="PD11" pad="58"/>
<connect gate="A" pin="PD12" pad="59"/>
<connect gate="A" pin="PD13" pad="60"/>
<connect gate="A" pin="PD14" pad="61"/>
<connect gate="A" pin="PD15" pad="62"/>
<connect gate="A" pin="PD2" pad="83"/>
<connect gate="A" pin="PD3" pad="84"/>
<connect gate="A" pin="PD4" pad="85"/>
<connect gate="A" pin="PD5" pad="86"/>
<connect gate="A" pin="PD6" pad="87"/>
<connect gate="A" pin="PD7" pad="88"/>
<connect gate="A" pin="PD8" pad="55"/>
<connect gate="A" pin="PD9" pad="56"/>
<connect gate="A" pin="PE0" pad="97"/>
<connect gate="A" pin="PE1" pad="98"/>
<connect gate="A" pin="PE10" pad="41"/>
<connect gate="A" pin="PE11" pad="42"/>
<connect gate="A" pin="PE12" pad="43"/>
<connect gate="A" pin="PE13" pad="44"/>
<connect gate="A" pin="PE14" pad="45"/>
<connect gate="A" pin="PE15" pad="46"/>
<connect gate="A" pin="PE2" pad="1"/>
<connect gate="A" pin="PE3" pad="2"/>
<connect gate="A" pin="PE4" pad="3"/>
<connect gate="A" pin="PE5" pad="4"/>
<connect gate="A" pin="PE6" pad="5"/>
<connect gate="A" pin="PE7" pad="38"/>
<connect gate="A" pin="PE8" pad="39"/>
<connect gate="A" pin="PE9" pad="40"/>
<connect gate="A" pin="VBAT" pad="6"/>
<connect gate="A" pin="VDDA" pad="22"/>
<connect gate="A" pin="VDD_1" pad="50"/>
<connect gate="A" pin="VDD_2" pad="75"/>
<connect gate="A" pin="VDD_3" pad="100"/>
<connect gate="A" pin="VDD_4" pad="28"/>
<connect gate="A" pin="VDD_5" pad="11"/>
<connect gate="A" pin="VREF+" pad="21"/>
<connect gate="A" pin="VREF-" pad="20"/>
<connect gate="A" pin="VSSA" pad="19"/>
<connect gate="A" pin="VSS_1" pad="49"/>
<connect gate="A" pin="VSS_2" pad="74"/>
<connect gate="A" pin="VSS_3" pad="99"/>
<connect gate="A" pin="VSS_4" pad="27"/>
<connect gate="A" pin="VSS_5" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="STM32F107VCT6"/>
<attribute name="OC_FARNELL" value="1737141"/>
<attribute name="OC_NEWARK" value="25R9446"/>
<attribute name="PACKAGE" value="LQFP-100"/>
<attribute name="SUPPLIER" value="STMicroelectronics"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F745VG">
<gates>
<gate name="G$1" symbol="STM32F745VG"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X160-100N">
<connects>
<connect gate="G$1" pin="BOOT0" pad="94"/>
<connect gate="G$1" pin="NRST" pad="14"/>
<connect gate="G$1" pin="OSC_IN" pad="12"/>
<connect gate="G$1" pin="OSC_OUT" pad="13"/>
<connect gate="G$1" pin="PA0-WKUP" pad="22"/>
<connect gate="G$1" pin="PA1" pad="23"/>
<connect gate="G$1" pin="PA14" pad="76"/>
<connect gate="G$1" pin="PA15" pad="77"/>
<connect gate="G$1" pin="PA2" pad="24"/>
<connect gate="G$1" pin="PA3" pad="25"/>
<connect gate="G$1" pin="PA4" pad="28"/>
<connect gate="G$1" pin="PA5" pad="29"/>
<connect gate="G$1" pin="PA6" pad="30"/>
<connect gate="G$1" pin="PA7" pad="31"/>
<connect gate="G$1" pin="PA_10" pad="69"/>
<connect gate="G$1" pin="PA_11" pad="70"/>
<connect gate="G$1" pin="PA_12" pad="71"/>
<connect gate="G$1" pin="PA_13" pad="72"/>
<connect gate="G$1" pin="PA_8" pad="67"/>
<connect gate="G$1" pin="PA_9" pad="68"/>
<connect gate="G$1" pin="PB0" pad="34"/>
<connect gate="G$1" pin="PB1" pad="35"/>
<connect gate="G$1" pin="PB10" pad="46"/>
<connect gate="G$1" pin="PB11" pad="47"/>
<connect gate="G$1" pin="PB12" pad="51"/>
<connect gate="G$1" pin="PB13" pad="52"/>
<connect gate="G$1" pin="PB14" pad="53"/>
<connect gate="G$1" pin="PB15" pad="54"/>
<connect gate="G$1" pin="PB2" pad="36"/>
<connect gate="G$1" pin="PB3" pad="89"/>
<connect gate="G$1" pin="PB4" pad="90"/>
<connect gate="G$1" pin="PB5" pad="91"/>
<connect gate="G$1" pin="PB6" pad="92"/>
<connect gate="G$1" pin="PB7" pad="93"/>
<connect gate="G$1" pin="PB8" pad="95"/>
<connect gate="G$1" pin="PB9" pad="96"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC10" pad="78"/>
<connect gate="G$1" pin="PC11" pad="79"/>
<connect gate="G$1" pin="PC12" pad="80"/>
<connect gate="G$1" pin="PC13-TAMPER-RTC" pad="7"/>
<connect gate="G$1" pin="PC14-OSC32_IN" pad="8"/>
<connect gate="G$1" pin="PC15-OSC32_OUT" pad="9"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="32"/>
<connect gate="G$1" pin="PC5" pad="33"/>
<connect gate="G$1" pin="PC6" pad="63"/>
<connect gate="G$1" pin="PC7" pad="64"/>
<connect gate="G$1" pin="PC8" pad="65"/>
<connect gate="G$1" pin="PC9" pad="66"/>
<connect gate="G$1" pin="PD0" pad="81"/>
<connect gate="G$1" pin="PD1" pad="82"/>
<connect gate="G$1" pin="PD10" pad="57"/>
<connect gate="G$1" pin="PD11" pad="58"/>
<connect gate="G$1" pin="PD12" pad="59"/>
<connect gate="G$1" pin="PD13" pad="60"/>
<connect gate="G$1" pin="PD14" pad="61"/>
<connect gate="G$1" pin="PD15" pad="62"/>
<connect gate="G$1" pin="PD2" pad="83"/>
<connect gate="G$1" pin="PD3" pad="84"/>
<connect gate="G$1" pin="PD4" pad="85"/>
<connect gate="G$1" pin="PD5" pad="86"/>
<connect gate="G$1" pin="PD6" pad="87"/>
<connect gate="G$1" pin="PD7" pad="88"/>
<connect gate="G$1" pin="PD8" pad="55"/>
<connect gate="G$1" pin="PD9" pad="56"/>
<connect gate="G$1" pin="PE0" pad="97"/>
<connect gate="G$1" pin="PE1" pad="98"/>
<connect gate="G$1" pin="PE10" pad="40"/>
<connect gate="G$1" pin="PE11" pad="41"/>
<connect gate="G$1" pin="PE12" pad="42"/>
<connect gate="G$1" pin="PE13" pad="43"/>
<connect gate="G$1" pin="PE14" pad="44"/>
<connect gate="G$1" pin="PE15" pad="45"/>
<connect gate="G$1" pin="PE2" pad="1"/>
<connect gate="G$1" pin="PE3" pad="2"/>
<connect gate="G$1" pin="PE4" pad="3"/>
<connect gate="G$1" pin="PE5" pad="4"/>
<connect gate="G$1" pin="PE6" pad="5"/>
<connect gate="G$1" pin="PE7" pad="37"/>
<connect gate="G$1" pin="PE8" pad="38"/>
<connect gate="G$1" pin="PE9" pad="39"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCAP1" pad="48"/>
<connect gate="G$1" pin="VCAP2" pad="73"/>
<connect gate="G$1" pin="VDDA" pad="21"/>
<connect gate="G$1" pin="VDD_1" pad="11"/>
<connect gate="G$1" pin="VDD_2" pad="27"/>
<connect gate="G$1" pin="VDD_3" pad="50"/>
<connect gate="G$1" pin="VDD_4" pad="75"/>
<connect gate="G$1" pin="VDD_5" pad="100"/>
<connect gate="G$1" pin="VREF+" pad="20"/>
<connect gate="G$1" pin="VSSA" pad="19"/>
<connect gate="G$1" pin="VSS_1" pad="10"/>
<connect gate="G$1" pin="VSS_2" pad="26"/>
<connect gate="G$1" pin="VSS_3" pad="49"/>
<connect gate="G$1" pin="VSS_4" pad="74"/>
<connect gate="G$1" pin="VSS_5" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F446XCXE">
<gates>
<gate name="G$1" symbol="STM32F445XCXE"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X160-100N">
<connects>
<connect gate="G$1" pin="BOOT0" pad="94"/>
<connect gate="G$1" pin="NRST" pad="14"/>
<connect gate="G$1" pin="OSC_IN" pad="12"/>
<connect gate="G$1" pin="OSC_OUT" pad="13"/>
<connect gate="G$1" pin="PA0-WKUP" pad="23"/>
<connect gate="G$1" pin="PA1" pad="24"/>
<connect gate="G$1" pin="PA14" pad="76"/>
<connect gate="G$1" pin="PA15" pad="77"/>
<connect gate="G$1" pin="PA2" pad="25"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PA4" pad="29"/>
<connect gate="G$1" pin="PA5" pad="30"/>
<connect gate="G$1" pin="PA6" pad="31"/>
<connect gate="G$1" pin="PA7" pad="32"/>
<connect gate="G$1" pin="PA_10" pad="69"/>
<connect gate="G$1" pin="PA_11" pad="70"/>
<connect gate="G$1" pin="PA_12" pad="71"/>
<connect gate="G$1" pin="PA_13" pad="72"/>
<connect gate="G$1" pin="PA_8" pad="67"/>
<connect gate="G$1" pin="PA_9" pad="68"/>
<connect gate="G$1" pin="PB0" pad="35"/>
<connect gate="G$1" pin="PB1" pad="36"/>
<connect gate="G$1" pin="PB10" pad="47"/>
<connect gate="G$1" pin="PB11/VCAP1" pad="48"/>
<connect gate="G$1" pin="PB12" pad="51"/>
<connect gate="G$1" pin="PB13" pad="52"/>
<connect gate="G$1" pin="PB14" pad="53"/>
<connect gate="G$1" pin="PB15" pad="54"/>
<connect gate="G$1" pin="PB2" pad="37"/>
<connect gate="G$1" pin="PB3" pad="89"/>
<connect gate="G$1" pin="PB4" pad="90"/>
<connect gate="G$1" pin="PB5" pad="91"/>
<connect gate="G$1" pin="PB6" pad="92"/>
<connect gate="G$1" pin="PB7" pad="93"/>
<connect gate="G$1" pin="PB8" pad="95"/>
<connect gate="G$1" pin="PB9" pad="96"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC10" pad="78"/>
<connect gate="G$1" pin="PC11" pad="79"/>
<connect gate="G$1" pin="PC12" pad="80"/>
<connect gate="G$1" pin="PC13-TAMPER-RTC" pad="7"/>
<connect gate="G$1" pin="PC14-OSC32_IN" pad="8"/>
<connect gate="G$1" pin="PC15-OSC32_OUT" pad="9"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="33"/>
<connect gate="G$1" pin="PC5" pad="34"/>
<connect gate="G$1" pin="PC6" pad="63"/>
<connect gate="G$1" pin="PC7" pad="64"/>
<connect gate="G$1" pin="PC8" pad="65"/>
<connect gate="G$1" pin="PC9" pad="66"/>
<connect gate="G$1" pin="PD0" pad="81"/>
<connect gate="G$1" pin="PD1" pad="82"/>
<connect gate="G$1" pin="PD10" pad="57"/>
<connect gate="G$1" pin="PD11" pad="58"/>
<connect gate="G$1" pin="PD12" pad="59"/>
<connect gate="G$1" pin="PD13" pad="60"/>
<connect gate="G$1" pin="PD14" pad="61"/>
<connect gate="G$1" pin="PD15" pad="62"/>
<connect gate="G$1" pin="PD2" pad="83"/>
<connect gate="G$1" pin="PD3" pad="84"/>
<connect gate="G$1" pin="PD4" pad="85"/>
<connect gate="G$1" pin="PD5" pad="86"/>
<connect gate="G$1" pin="PD6" pad="87"/>
<connect gate="G$1" pin="PD7" pad="88"/>
<connect gate="G$1" pin="PD8" pad="55"/>
<connect gate="G$1" pin="PD9" pad="56"/>
<connect gate="G$1" pin="PE0" pad="97"/>
<connect gate="G$1" pin="PE1" pad="98"/>
<connect gate="G$1" pin="PE10" pad="41"/>
<connect gate="G$1" pin="PE11" pad="42"/>
<connect gate="G$1" pin="PE12" pad="43"/>
<connect gate="G$1" pin="PE13" pad="44"/>
<connect gate="G$1" pin="PE14" pad="45"/>
<connect gate="G$1" pin="PE15" pad="46"/>
<connect gate="G$1" pin="PE2" pad="1"/>
<connect gate="G$1" pin="PE3" pad="2"/>
<connect gate="G$1" pin="PE4" pad="3"/>
<connect gate="G$1" pin="PE5" pad="4"/>
<connect gate="G$1" pin="PE6" pad="5"/>
<connect gate="G$1" pin="PE7" pad="38"/>
<connect gate="G$1" pin="PE8" pad="39"/>
<connect gate="G$1" pin="PE9" pad="40"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCAP2" pad="73"/>
<connect gate="G$1" pin="VDDA" pad="22"/>
<connect gate="G$1" pin="VDD_0" pad="100"/>
<connect gate="G$1" pin="VDD_1" pad="11"/>
<connect gate="G$1" pin="VDD_2" pad="19"/>
<connect gate="G$1" pin="VDD_3" pad="28"/>
<connect gate="G$1" pin="VDD_4" pad="50"/>
<connect gate="G$1" pin="VDD_5" pad="75"/>
<connect gate="G$1" pin="VREF+" pad="21"/>
<connect gate="G$1" pin="VSSA/VREF-" pad="20"/>
<connect gate="G$1" pin="VSS_1" pad="10"/>
<connect gate="G$1" pin="VSS_2" pad="27"/>
<connect gate="G$1" pin="VSS_3" pad="49"/>
<connect gate="G$1" pin="VSS_4" pad="74"/>
<connect gate="G$1" pin="VSS_5" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16244" prefix="IC">
<description>16-bit &lt;B&gt;BUFFER/LINE DRIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416244"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1G" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="2"/>
<connect gate="G$1" pin="1Y2" pad="3"/>
<connect gate="G$1" pin="1Y3" pad="5"/>
<connect gate="G$1" pin="1Y4" pad="6"/>
<connect gate="G$1" pin="2A1" pad="41"/>
<connect gate="G$1" pin="2A2" pad="40"/>
<connect gate="G$1" pin="2A3" pad="38"/>
<connect gate="G$1" pin="2A4" pad="37"/>
<connect gate="G$1" pin="2G" pad="48"/>
<connect gate="G$1" pin="2Y1" pad="8"/>
<connect gate="G$1" pin="2Y2" pad="9"/>
<connect gate="G$1" pin="2Y3" pad="11"/>
<connect gate="G$1" pin="2Y4" pad="12"/>
<connect gate="G$1" pin="3A1" pad="36"/>
<connect gate="G$1" pin="3A2" pad="35"/>
<connect gate="G$1" pin="3A3" pad="33"/>
<connect gate="G$1" pin="3A4" pad="32"/>
<connect gate="G$1" pin="3G" pad="25"/>
<connect gate="G$1" pin="3Y1" pad="13"/>
<connect gate="G$1" pin="3Y2" pad="14"/>
<connect gate="G$1" pin="3Y3" pad="16"/>
<connect gate="G$1" pin="3Y4" pad="17"/>
<connect gate="G$1" pin="4A1" pad="30"/>
<connect gate="G$1" pin="4A2" pad="29"/>
<connect gate="G$1" pin="4A3" pad="27"/>
<connect gate="G$1" pin="4A4" pad="26"/>
<connect gate="G$1" pin="4G" pad="24"/>
<connect gate="G$1" pin="4Y1" pad="19"/>
<connect gate="G$1" pin="4Y2" pad="20"/>
<connect gate="G$1" pin="4Y3" pad="22"/>
<connect gate="G$1" pin="4Y4" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP" package="TSSOP48">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1G" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="2"/>
<connect gate="G$1" pin="1Y2" pad="3"/>
<connect gate="G$1" pin="1Y3" pad="5"/>
<connect gate="G$1" pin="1Y4" pad="6"/>
<connect gate="G$1" pin="2A1" pad="41"/>
<connect gate="G$1" pin="2A2" pad="40"/>
<connect gate="G$1" pin="2A3" pad="38"/>
<connect gate="G$1" pin="2A4" pad="37"/>
<connect gate="G$1" pin="2G" pad="48"/>
<connect gate="G$1" pin="2Y1" pad="8"/>
<connect gate="G$1" pin="2Y2" pad="9"/>
<connect gate="G$1" pin="2Y3" pad="11"/>
<connect gate="G$1" pin="2Y4" pad="12"/>
<connect gate="G$1" pin="3A1" pad="36"/>
<connect gate="G$1" pin="3A2" pad="35"/>
<connect gate="G$1" pin="3A3" pad="33"/>
<connect gate="G$1" pin="3A4" pad="32"/>
<connect gate="G$1" pin="3G" pad="25"/>
<connect gate="G$1" pin="3Y1" pad="13"/>
<connect gate="G$1" pin="3Y2" pad="14"/>
<connect gate="G$1" pin="3Y3" pad="16"/>
<connect gate="G$1" pin="3Y4" pad="17"/>
<connect gate="G$1" pin="4A1" pad="30"/>
<connect gate="G$1" pin="4A2" pad="29"/>
<connect gate="G$1" pin="4A3" pad="27"/>
<connect gate="G$1" pin="4A4" pad="26"/>
<connect gate="G$1" pin="4G" pad="24"/>
<connect gate="G$1" pin="4Y1" pad="19"/>
<connect gate="G$1" pin="4Y2" pad="20"/>
<connect gate="G$1" pin="4Y3" pad="22"/>
<connect gate="G$1" pin="4Y4" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP-12-MODULE_WIFI">
<gates>
<gate name="G$1" symbol="ESP-12-WIFI_MODULE"/>
</gates>
<devices>
<device name="" package="ESP-12-WIFI_MODULE">
<connects>
<connect gate="G$1" pin="ADC" pad="P$2"/>
<connect gate="G$1" pin="CS0" pad="P$9"/>
<connect gate="G$1" pin="EN" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$15"/>
<connect gate="G$1" pin="GPIO0" pad="P$18"/>
<connect gate="G$1" pin="GPIO10" pad="P$12"/>
<connect gate="G$1" pin="GPIO12" pad="P$6"/>
<connect gate="G$1" pin="GPIO13" pad="P$7"/>
<connect gate="G$1" pin="GPIO14" pad="P$5"/>
<connect gate="G$1" pin="GPIO15" pad="P$16"/>
<connect gate="G$1" pin="GPIO16" pad="P$4"/>
<connect gate="G$1" pin="GPIO2" pad="P$17"/>
<connect gate="G$1" pin="GPIO4" pad="P$19"/>
<connect gate="G$1" pin="GPIO5" pad="P$20"/>
<connect gate="G$1" pin="GPIO9" pad="P$11"/>
<connect gate="G$1" pin="MISO" pad="P$10"/>
<connect gate="G$1" pin="MOSI" pad="P$13"/>
<connect gate="G$1" pin="RST" pad="P$1"/>
<connect gate="G$1" pin="RXD0" pad="P$21"/>
<connect gate="G$1" pin="SCLK" pad="P$14"/>
<connect gate="G$1" pin="TXD0" pad="P$22"/>
<connect gate="G$1" pin="VCC" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5VSB" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5VSB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
